Synamedia MEG setup – **HSN**

HSN2 HD MP4 TSoip Out

**Task-** Configuring Synamedia MEG IRDs

**Condition-** Service Routing HSN2 HD MP4 - TSoip Out

**Standard-** How to configure a Synamedia MEG IRD for Service Routing

**Action Items:**

* Service Routing HD MP4
	+ Begin by **Browsing to IP** of MEG IRD (Default ip - 192.168.2.20)
		- **Enter UN & PW** *(see figure 1) (UN: Admin ; PW: Password)*

*Figure 1 - Login*



* Click on **Add New Channel** *(see figure 2)*

Figure 2 – Add Channel



* + Choose which option you would like to do
		- Select **Service Routing** for TSoip setup *(see figure 3)*

Figure 3 – Service Routing



* + Service Routing – TSoip
		- Select **Use Existing Input**
		- **Input Selection - DVB-S2:DVBS2 1 (4.08GHz)**
		- Select which **Service ID** you would like to Service Route by choosing the service in the **Dropdown Menu - (23) for HSN2 HD** *(see figure 4)*

Figure 4 – Service Routing Input Options



* **Descrambling - Disabled**
* Click on **Output** next
	+ Select **Type**
		- Select **Xgress**
			* Select Xgress port you would like to use (Port-1)
			* Host 225.1.1.2
			* UDP 49153
			* Leave the remaining fields as default
	+ Tick **Service ID** box
		- Enter **Service ID – 23** *(see figure 5)*

*Figure 5 – Configure Output*

**

* Click on **Create** in upper right corner (*see figure 6)*

*Figure 6 – Create and Finish*



* *You should see a popup box that says* ***“Channel activated successfully”***
* **Setup complete** –There should now be 1 channel with a green checkmark *(see figure 7)*

Figure 7 – Channel Created



\*Advanced View configurations are beyond the scope of this document.